Chip back potential is the level which bulk silicon is maintained by on-chip connection, or it is the level to which the chip back must be connected when specifically stated below. If no potential is given the chip back should be isolated.

**.025”**



**.025”**

**Top Material: Al**

**Backside Material: Au**

**Bond Pad Size: .004 X .004” Min**

**Backside Potential:**

**Mask Ref: GC**

**APPROVED BY: DK DIE SIZE .025” X .025” DATE: 1/26/22**

**MFG: RAYTHEON THICKNESS .000” P/N: 2N2102**

**DG 10.1.2**

#### Rev B, 7/1