Chip back potential is the level which bulk silicon is maintained by on-chip connection, or it is the level to which the chip back must be connected when specifically stated below. If no potential is given the chip back should be isolated.



**Top Material: Al**

**Backside Material: Au**

**Bond Pad Size: .005” X .005”**

**Backside Potential: Collector**

**Mask Ref:**

**APPROVED BY: DK DIE SIZE .026” X .026” DATE: 5/5/22**

**MFG: ZETEX THICKNESS .006” P/N: 2N3637**

**DG 10.1.2**

#### Rev B, 7/19/02