
Chip back potential is the level which bulk silicon is maintained by on-chip connection, or it is the level to which the chip back must be connected when specifically stated below. If no potential is given the chip back should be isolated.

**.129”**

**PAD FUNCTIONS:**

1. **V IN (2 bond pads)**
2. **V OUT (2 bond pads)**
3. **V OUT SENSE**
4. **ADJUST**



**Top Material: Al**

**Backside Material: Au**

**Bond Pad Size: .004 X .004”**

**Backside Potential: GATE**

**Mask Ref: F132**

**APPROVED BY: DK DIE SIZE .022” X .022” DATE: 12/20/22**

**MFG: INTERFET THICKNESS .010” P/N: 2N4392**

**DG 10.1.2**

#### Rev B, 7/1