Chip back potential is the level which bulk silicon is maintained by on-chip connection, or it is the level to which the chip back must be connected when specifically stated below. If no potential is given the chip back should be isolated.

**PAD FUNCTONS:**

1. **1A**
2. **1B**
3. **2A**
4. **2B**
5. **2C**
6. **2Y**
7. **GND**
8. **3Y**
9. **3A**
10. **3B**
11. **3C**
12. **1Y**
13. **1C**
14. **VCC**

**DRAFT**

**.042”**

**L**

**O**

**1**

**1**

**Z**

**MASK**

**REF**

**.042”**

**Top Material: Al**

**Backside Material: Si**

**Bond Pad Size: .004” X .004”**

**Backside Potential: GND**

**Mask Ref: LO11Z**

**APPROVED BY: DK DIE SIZE .042” X .042” DATE: 4/19/21**

**MFG: FAIRCHILD THICKNESS .015” P/N: 54LS11**

**DG 10.1.2**

#### Rev B, 7/1