Chip back potential is the level which bulk silicon is maintained by on-chip connection, or it is the level to which the chip back must be connected when specifically stated below. If no potential is given the chip back should be isolated.



**Top Material: Al**

**Backside Material: Si**

**Bond Pad Size: .00394” X .00394”**

**Backside Potential: Floating**

**Mask Ref:**

**APPROVED BY: DK DIE SIZE .079” X .098” DATE: 9/9/21**

**MFG: TEXAS INSTRUMENTS THICKNESS .025” P/N: SN65C1168**

**DG 10.1.2**

#### Rev B, 7/19/02