Chip back potential is the level which bulk silicon is maintained by on-chip connection, or it is the level to which the chip back must be connected when specifically stated below. If no potential is given the chip back should be isolated.

****

****

**Top Material: Al**

**Backside Material: Si**

**Bond Pad Size: .004 x .004”**

**Backside Potential: Unbiased**

**Mask Ref: A38741**

**APPROVED BY: DK DIE SIZE .056” X .069” DATE: 8/25/21**

**MFG: HARRIS / INTERSIL THICKNESS .019” P/N: HA0-2605**

**DG 10.1.2**

#### Rev B, 7/1