Chip back potential is the level which bulk silicon is maintained by on-chip connection, or it is the level to which the chip back must be connected when specifically stated below. If no potential is given the chip back should be isolated.

**PAD FUNCTIONS:**

1. **OUTPUT 1**
2. **INPUT 1 –**
3. **INPUT 1 +**
4. **V +**
5. **INPUT 2 +**
6. **INPUT 2 -**
7. **OUTPUT 2**
8. **OUTPUT 3**
9. **INPUT 3 -**
10. **INPUT 3 +**
11. **GND**
12. **INPUT 4 +**
13. **INPUT 4 –**
14. **OUTPUT 4**

**.050”**

 **11**

 **4**

**5**

**6**

**7**

**8**

**9**

**10**

**3**

**2**

**1**

**14**

**13**

**12**

**MASK**

**REF**

**U242**

**.047”**

**Top Material: Al**

**Backside Material: Si**

**Bond Pad Size: .0035” X .0035”**

**Backside Potential: FLOATING**

**Mask Ref: U242**

**APPROVED BY: DK DIE SIZE .047” X .050” DATE: 12/14/22**

**MFG: SILICON SUPPLIES THICKNESS .011” P/N: LM124**

**DG 10.1.2**

#### Rev B, 7/1